Run C9SETROM.EXE from Real DOS mode to reset the card's Serial EEPROM to
default values. Use when the card is not detected properly by Plug&Play BIOS
or Device Manager shows device failure.
If the program exits without write, remove EN_PNP jumper from the card and try
again. Then put the jumper back. (Move the jumper with POWER OFF)