Run C9SETROM.EXE from Real DOS mode to disable IRQ and DMA of the WSS device
and disable IRQ for the External MIDI/Dream Wavetable MIDI. This will disable
the WSS device. The Dream Wavetable MIDI does not need the IRQ and will work
properly. This file also allocates 388-38B address range to the SB16 device so
running Add New Hardware wizard will not detect phantom AdLib card.

If the program exits without write, remove EN_PNP jumper from the card and try
again. Then put the jumper back. (Move the jumper with POWER OFF)

Do NOT run WEINIT.EXE if the resources are modified by this program. If you run
it, saving the settings will corrupt the Serial EEPROM and you will need to
reset it using either this program or the one in PNPFIX directory.

To enable the WSS device and MIDI IRQ again, use C9SETROM.EXE in PNPFIX
directory.